Circuit: * D:\Flo\CloudStation\Projekte\Postkastl\Schematic-Sim\Postkasten.asc

Per .tran options, skipping operating point for transient analysis.

Date: Fri Jan 20 22:09:43 2017
Total elapsed time: 0.117 seconds.

tnom = 27
temp = 27
method = modified trap
totiter = 20153
traniter = 20153
tranpoints = 10066
accept = 10056
rejected = 10
matrix size = 4
fillins = 0
solver = Normal
Matrix Compiler1: 154 bytes object code size  0.0/0.0/[0.0]
Matrix Compiler2: 262 bytes object code size  0.0/0.0/[0.0]


