{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["Sheet1"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Sheet1","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[]}
["Batterielebensdauer ESP8266 an 2x AA Alkaline-Batterie"]
[]
["Vorgaben"]
["typ. Auslösungen pro Tag",2]
["nutzbare Batteriekapazität",2000,"mAh"]
[]
["Messwerte ","mA"]
["Ruhezustand",1.2999999999999999E-2]
["booten",100]
["Verbindung aktiv, Daten senden",170]
["Verbindung aus, Programm aktiv, warten",15]
[]
["typischer Programmablauf","s","h","mAh"]
["booten",1,{"$f":"B14/3600","v":2.7777777777777778E-4},{"$f":"C14*B9","v":2.7777777777777776E-2}]
["Verbindung aktiv, Daten senden",6,{"$f":"B15/3600","v":1.6666666666666668E-3},{"$f":"C15*B10","v":0.28333333333333333}]
["Verbindung aus, Programm aktiv, warten",300,{"$f":"B16/3600","v":8.3333333333333329E-2},{"$f":"C16*B11","v":1.25}]
["pro Vorgang",{"$f":"SUM(B14:B16)","v":307},{"$f":"SUM(C14:C16)","v":8.5277777777777772E-2},{"$f":"ROUNDUP(SUM(D14:D16),2)","v":1.57}]
[]
[null,"s","h","mAh"]
["alle Vorgänge pro Tag",{"$f":"B4*B17","v":614},{"$f":"B20/3600","v":0.17055555555555554},{"$f":"ROUNDUP(D17*B4,2)","v":3.14}]
[]
["restlicher Tag",null,{"$f":"24-C20","v":23.829444444444444},{"$f":"ROUNDUP(B8*C22,2)","v":0.31}]
[]
[]
["Stromverbrauch pro Tag",null,null,{"$f":"D22+D20","v":3.45}," mAh"]
[]
["Batterielebensdauer",null,null,{"$f":"B5/D25","v":579.71014492753625}," Tage"]